{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Submittal Cover Sheet Final Dra","Menu","Component Categories"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Submittal Cover Sheet Final Dra","index":0,"n_rows":21,"n_cols":14,"rows_kept":21,"cut":false,"hidden":false,"merged":[[1,1,1,13],[13,1,13,7],[13,9,13,12],[14,9,14,12],[3,1,3,8],[8,9,8,10],[5,1,5,8],[3,10,5,13]]}
[]
[null,"PRODUCT DATA REPORTING FORM for LEED v5 Projects"]
[]
[null,"THIS FORM IS REQUIRED TO BE SUBMITTED WITH Product Data Submittals for LEED v5 Projects",null,null,null,null,null,null,null,null,{"$error":"#VALUE!"}]
[]
[null,"You must include backup documentation such as SPECIFIC Product Data Sheets, 3rd party certification, Cut Sheets, Product Specific Letter from Manufacturer, etc. (Not marketing material)"]
[null,"LEED Project Name:"]
[]
[null,"Subcontractor:"]
[]
[null,"Submittal Number:"]
[]
[]
[null,"Project Product Data",null,null,null,null,null,null,"Materials and Resources LEED Credits","Low-Emitting Materials LEED Credits"]
[null,null,null,null,null,null,null,null,"Building Product Selections and Procurement","Qualifying VOC Standards:\n CDPH Standard Method v1.2\n FloorScore: Hard Surfaces & Adhesives \n Green Label Plus: Carpet, Adhesive, Cushion \n UL Greengaurd Gold: When Meeting CDPH Std"]
[null,null,"Manufacturer","Product Name","Product Costs (only exclude labor) ($)","Quantity","Unit","Component Category","Select all that Apply\n(Need Help?)","CDPH Emissions\n testing compliant?\n (Yes/No)","VOC Content (g/L)","Wood Products are ULEF or NAF12?\n (Yes/No)","Wood Products are CARB exempt?\n (Yes/No)","Notes: "]
[null,1,"National Gypsum","XP Firesheild",10000,1000,"ft2","Insulation - Heavy Density Mineral Wool Board",null,"CDPHv1.2-2017",0,"No","No"]
[null,2,"Pabco","Type X",5000,250,"yd3","Insulation - Expanded Polystyrene Type I",null,"CDPHv1.2-2017",0,"No","No"]
[null,3,"Hilti","FS One",50,10,"gal","Fireproofing - Spray Applied Fireproofing Standard Density",null,"Not Available",32]
[null,4,null,null,null,null,"Select","Select",null,"N/A"]
[null,5,null,null,null,null,"Select","Select",null,"Select"]

{"sheet":"Menu","index":1,"n_rows":136,"n_cols":1,"rows_kept":136,"cut":false,"hidden":true,"merged":[[2,0,3,4],[15,0,15,4]]}
[]
[]
["Building Product Selections and Procurement Options"]
[]
["EPD"]
["EPD Optimized"]
["HPD"]
["Declare"]
["C2C"]
["C2C MHC"]
["Recycled Content"]
["FSC"]
[]
[]
[]
["Component Categories 2025 CLF"]
["Finishes - Gypsum Board 1/2in"]
["Finishes - Gypsum Board 5/8in"]
["Finishes - Glass Mat Gypsum Board 1/2in"]
["Finishes - Glass Mat Gypsum Board 5/8in"]
["Finishes - Acoustical Ceiling Tiles NRC 0.75"]
["Finishes - Acoustical Ceiling Tiles 0.75 NRC 0.90"]
["Finishes - Acoustical CeilingTiles NRC 0.90"]
["Finishes - Ceramic Tile"]
["Finishes - Homogeneous Vinyl Flooring"]
["Finishes - Heterogeneous Vinyl Flooring"]
["Finishes - Rubber Flooring"]
["Finishes - Luxury Vinyl Tile Glue Down"]
["Finishes - Luxury Vinyl Tile Loose Lay"]
["Finishes - Rigid Core Flooring SPC"]
["Finishes - Vinyl Composition Tile"]
["Insulation - Expanded Polystyrene Type I"]
["Insulation - Fiberglass Board"]
["Insulation - Heavy Density Mineral Wool Board"]
["Insulation - Polyiso Aluminum Foil Facer"]
["Insulation - Polyiso GRF Facer"]
["Insulation - Polyiso CGF Facer"]
["Insulation - Polyiso Wall"]
["Insulation - Polyiso Roof"]
["Insulation - Extruded Polystyrene Board 25 psi"]
["Insulation - Extruded Polystyrene Board 40 psi"]
["Insulation - Extruded Polystyrene Board 60 psi"]
["Insulation - Extruded Polystyrene Board 100 psi"]
["Insulation - Fiberglass Blanket"]
["Insulation - Mineral Wool Blanket"]
["Insulation - Blanket Insulation"]
["Insulation - Closed Cell Spray Polyurethane Foam Medium Density"]
["Insulation - Closed Cell Spray Polyurethane Foam Roofing"]
["Insulation - Open Cell Spray Polyurethane Foam"]
["Insulation - Mineral Wool Loose Fill"]
["Insulation - Fiberglass Loose Fill"]
["Insulation - Cellulose Loose Fill"]
["Insulation - Loose Fill Insulation All Types"]
["Fireproofing - Spray Applied Fireproofing Standard Density"]
["Fireproofing - Spray Applied Fireproofing Medium Density"]
["Fireproofing - Spray Applied Fireproofing High Density"]
["Openings - Flat Glass"]
["Concrete - Cement"]
["Concrete - Ready Mix"]
["Concrete - Shotcrete"]
["Masonry - CMUs"]
["Masonry - Brick"]
["Steel - Rebar"]
["Steel - Structural Steel Hot Rolled Unfabricated"]
["Steel - Structural Stee Hot Rolled Fabricated"]
["Steel - Structural Steel Plate Unfabricated"]
["Steel - Structural Steel Plate Fabricated"]
["Steel - Structural Steel HSS Unfabricated"]
["Steel - Structural Steel HSS Fabricated"]
["Steel - Cold Formed Steel Framing"]
["Steel - Steel Decking"]
["Steel - Open Web Steel Joists"]
["Aluminum - Extrusions Mill Finish"]
["Aluminum - Extrusions Anodized"]
["Aluminum - Extrusions Painted"]
["Aluminum - Extrusions Anodized Thermally Improved"]
["Aluminum - Extrusions Painted Thermally Improved"]
["Aluminum - Aluminum Sheet"]
["Cladding - Roll Formed Metal Panel Steel"]
["Cladding - Roll Formed Metal Panel Aluminum"]
["Cladding - Roll Formed Metal Panels"]
["Cladding - MCM Panel Aluminum"]
["Cladding - Insulated Metal Panel 2in Thick"]
["Cladding - Insulated Metal Panel 4in Thick"]
["Cladding - Insulated Metal Panel 6in Thick"]
["Cladding - Insulated Metal Panel User-Defined Thickness"]
["Membrane Roofing - Built Up Asphalt Roofing Hot Asphalt        "]
["Membrane Roofing - BUR Fastened Base 2 Ply Felts and Cap in Hot Asphalt"]
["Membrane Roofing - SBS Modified Bitumen Roofing Membrane Installation Cold Adhesive"]
["Membrane Roofing - SBS Modified Bitumen Roofing Membrane Installation Hot Asphalt"]
["Membrane Roofing - SBS Modified Bitumen Roofing Membrane Installation Hybrid Self-Adhered SBS Base Sheet and Torch-Applied SBS Cap"]
["Membrane Roofing - SBS Modified Bitumen Roofing Membrane Installation Self Adhered"]
["Membrane Roofing - SBS Modified Bitumen Roofing Membrane Installation Torch Applied"]
["Membrane Roofing - SBS Modified Bitumen Roofing Membrane"]
["Membrane Roofing - APP Modified Bitumen Roofing Membrane Installation Cold Adhesive"]
["Roofing - APP modified bitumen roofing membrane installation torch applied"]
["Roofing - APP modified bitumen roofing membrane"]
["Roofing - SBS/APP modified bitumen roofing membrane hybrid self-adhered SBS base sheet and torch-applied APP"]
["Roofing - Single ply PVC membrane roofing 40 mils"]
["Roofing - Single ply PVC membrane roofing 48 mils"]
["Roofing - Single ply PVC membrane roofing 60 mils"]
["Roofing - ingle ply PVC membrane roofing 80 mils"]
["Roofing - TPO membrane roofing 45 mil"]
["Roofing - TPO membrane roofing 60 mil"]
["Roofing - TPO membrane roofing 80 mil"]
["Roofing - EPDM membrane roofing reinforced 45 mil"]
["Roofing - EPDM membrane roofing reinforced 60 mil"]
["Roofing - EPDM membrane roofing reinforced 75 mil"]
["Roofing - EPDM membrane roofing non-reinforced 45 mil"]
["Roofing - EPDM membrane roofing non-reinforced 60 mil"]
["Roofing - EPDM membrane roofing non-reinforced 90 mil"]
["Roofing - Asphalt Shingles"]
["Asphalt - Aspalt Mixtures"]
["Wood - Softwood Lumber"]
["Wood - Softwood Lumber U.S. Inland Northwest"]
["Wood - Softwood Lumber U.S. Southern"]
["Wood - Softwood Lumber U.S. Pacific Coast"]
["Wood - Softwood Lumber British Columbia"]
["Wood - Redwood Lumber"]
["Wood - Laminated Strand Lumber"]
["Wood - Laminated Veneer Lumber "]
["Wood - CLT North America"]
["Wood - CLT British Columbia"]
["Wood - CLT Eastern Canada"]
["Wood - CLT Southern US"]
["Wood - CLT Western US"]
["Wood - Mass Ply Panel"]
["Wood - Dowel Laminated Timber"]
["Wood - GLT"]
["Wood - GLT British Columbia"]
["Wood - Softwood Plywood"]
["Wood - Softwood Plywood British Columbia"]
["Wood - Oriented Strandboard"]
["Wood - Wood Sheathing Plywood and OSB"]
["Wood - Wood I Joist 300mm"]
["Select"]

{"sheet":"Component Categories","index":2,"n_rows":371,"n_cols":5,"rows_kept":371,"cut":false,"hidden":false,"merged":[[1,1,1,4]]}
[]
[null,"2025 CLF Material Baselines per Component Category"]
[null,"Category","Product type; additional description","Baseline value (kg CO2e / declared unit)","Declared unit"]
[null,"Gypsum board ","Gypsum board, 1/2 in",207,"1000 ft2 (92.9 m2)"]
[null,"Gypsum board ","Gypsum board, 5/8 in",277,"1001 ft2 (92.9 m2)"]
[null,"Glass-mat gypsum board ","Glass-mat gypsum board, 1/2 in",437,"1002 ft2 (92.9 m2)"]
[null,"Glass-mat gypsum board ","Glass-mat gypsum board, 5/8 in",504,"1003 ft2 (92.9 m2)"]
[null,"Acoustical ceiling tiles ","ACT, NRC < 0.75",0.45,"1 ft2"]
[null,"Acoustical ceiling tiles ","ACT, 0.75 ≤ NRC ≤ 0.90",2.1,"1 ft2"]
[null,"Acoustical ceiling tiles ","ACT, NRC > 0.90",2.8,"1 ft2"]
[null,"Tile","Ceramic tile",14.1,"1 m2"]
[null,"Resilient flooring ","Homogeneous vinyl flooring",7.48,"1 m2"]
[null,"Resilient flooring ","Heterogeneous vinyl flooring",5.87,"1 m2"]
[null,"Resilient flooring ","Rubber flooring, ≅3.2 mm",10.8,"1 m2"]
[null,"Resilient flooring ","Luxury vinyl tile (LVT), glue down",9.7799999999999994,"1 m2"]
[null,"Resilient flooring ","Luxury vinyl tile (LVT), loose lay",11.6,"1 m2"]
[null,"Resilient flooring ","Rigid core flooring, SPC",8.24,"1 m2"]
[null,"Resilient flooring ","Vinyl composition tile (VCT)",4.63,"1 m2"]
[null,"Cement","Portland cement, USA",919,"1 metric ton"]
[null,"Cement","Portland cement, USA",919,"1 metric ton"]
[null,"Cement","Blended hydraulic cement, USA",739,"1 metric ton"]
[null,"Cement","Portland-limestone cement, USA",844,"1 metric ton"]
[null,"Cement","Hydraulic cement, USA (portland, portland-limestone, and blended hydraulic cements)",873,"1 metric ton"]
[null,"Cement","GU cement, Western Canada",796,"1 metric ton"]
[null,"Cement","GU cement, Central Canada",854,"1 metric ton"]
[null,"Cement","GU cement, Eastern Canada",898,"1 metric ton"]
[null,"Cement","GUL cement, Western Canada",732,"1 metric ton"]
[null,"Cement","GUL cement, Central Canada",798,"1 metric ton"]
[null,"Cement","GUL cement, Eastern Canada",864,"1 metric ton"]
[null,"Cement","Masonry cement",587,"1 metric ton"]
[null,"Cement","Slag cement",147,"1 metric ton"]
[null,"Ready-mix","Ready-mixed concrete, USA, National, 2500 psi",240,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, National, 3000 psi",262,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, National, 4000 psi",308,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, National, 5000 psi",365,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, National, 6000 psi",385,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, National, 8000 psi",446,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, National, LW 3000 psi",492,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, National, LW 4000 psi",540,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, National, LW 5000 psi",588,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Southwest, 2500 psi",257,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Southwest, 3000 psi",279,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Southwest, 4000 psi",323,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Southwest, 5000 psi",378,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Southwest, 6000 psi",401,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Southwest, 8000 psi",456,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Southwest, 9000 psi",437,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Southwest, 10,000 psi",471,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Southwest, LW 3000 psi",500,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Southwest, LW 4000 psi",546,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Southwest, LW 5000 psi",594,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Northwest, 2500 psi",235,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Northwest, 3000 psi",261,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Northwest, 4000 psi",316,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Northwest, 5000 psi",386,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Northwest, 6000 psi",408,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Northwest, 8000 psi",487,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Northwest, 9000 psi",378,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Northwest, 10,000 psi",470,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Northwest, LW 3000 psi",518,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Northwest, LW 4000 psi",575,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Pacific Northwest, LW 5000 psi",632,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Rocky Mountains, 2500 psi",232,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Rocky Mountains, 3000 psi",255,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Rocky Mountains, 4000 psi",301,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Rocky Mountains, 5000 psi",358,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Rocky Mountains, 6000 psi",379,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Rocky Mountains, 8000 psi",440,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Rocky Mountains, 10,000 psi",387,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Rocky Mountains, LW 3000 psi",484,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Rocky Mountains, LW 4000 psi",532,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Rocky Mountains, LW 5000 psi",580,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, South Central, 2500 psi",226,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, South Central, 3000 psi",245,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, South Central, 4000 psi",286,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, South Central, 5000 psi",336,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, South Central, 6000 psi",356,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, South Central, 8000 psi",409,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, South Central, LW 3000 psi",468,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, South Central, LW 4000 psi",510,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, South Central, LW 5000 psi",555,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, North Central, 2500 psi",241,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, North Central, 3000 psi",264,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, North Central, 4000 psi",312,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, North Central, 5000 psi",372,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, North Central, 6000 psi",394,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, North Central, 8000 psi",460,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, North Central, LW 3000 psi",487,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, North Central, LW 4000 psi",537,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, North Central, LW 5000 psi",591,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Southeastern, 2500 psi",247,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Southeastern, 3000 psi",268,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Southeastern, 4000 psi",309,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Southeastern, 5000 psi",360,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Southeastern, 6000 psi",382,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Southeastern, 8000 psi",435,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Southeastern, 9000 psi",534,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Southeastern, 10,000 psi",609,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Southeastern, 12,000 psi",593,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Southeastern, LW 3000 psi",478,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Southeastern, LW 4000 psi",521,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Southeastern, LW 5000 psi",562,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Great Lakes, 2500 psi",232,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Great Lakes, 3000 psi",255,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Great Lakes, 4000 psi",303,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Great Lakes, 5000 psi",363,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Great Lakes, 6000 psi",383,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Great Lakes, 8000 psi",452,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Great Lakes, LW 3000 psi",499,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Great Lakes, LW 4000 psi",551,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Great Lakes, LW 5000 psi",603,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Eastern, 2500 psi",240,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Eastern, 3000 psi",264,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Eastern, 4000 psi",314,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Eastern, 5000 psi",378,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Eastern, 6000 psi",399,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Eastern, 8000 psi",472,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Eastern, 9000 psi",410,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Eastern, 10,000 psi",429,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Eastern, 12,000 psi",353,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Eastern, LW 3000 psi",517,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Eastern, LW 4000 psi",573,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, USA, Eastern, LW 5000 psi",628,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 15 MPa, w/o AEAs",179,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 20 MPa, w/ AEAs",194,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 20 MPa, w/o AEAs",195,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 25 MPa",231,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 25 MPa, w/o AEAs",220,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 30 MPa",270,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 30 MPa, w/o AEAs",259,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 32 MPa",285,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 32 MPa, w/o AEAs",272,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 35 MPa",311,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 35 MPa, w/o AEAs",294,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 40 MPa",344,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 40 MPa, w/o AEAs",329,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 45 MPa",356,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 45 MPa, w/o AEAs",335,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 50 MPa",345,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 50 MPa, w/o AEAs",359,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 55 MPa",402,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 55 MPa, w/o AEAs",377,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 60 MPa",422,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, British Columbia, 60 MPa, w/o AEAs",400,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 20 MPa",273,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 20 MPa, w/o AEAs",261,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 25 MPa",318,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 25 MPa, w/o AEAs",306,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 30 MPa",369,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 30 MPa, w/o AEAs",334,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 32 MPa",397,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 32 MPa, w/o AEAs",314,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 35 MPa",410,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 35 MPa, w/o AEAs",328,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 40 MPa",427,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 40 MPa, w/o AEAs",418,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 45 MPa",465,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 50 MPa",488,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 50 MPa, w/o AEAs",447,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Alberta, 55 MPa",466,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Saskatchewan, 25 MPa",313,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Saskatchewan, 25 MPa, w/o AEAs",296,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Saskatchewan, 30 MPa",346,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Saskatchewan, 30 MPa, w/o AEAs",317,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Saskatchewan, 32 MPa",380,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Saskatchewan, 32 MPa, w/o AEAs",338,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Saskatchewan, 35 MPa",417,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Saskatchewan, 35 MPa, w/o AEAs",358,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Saskatchewan, 40 MPa",442,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Saskatchewan, 40 MPa, w/o AEAs",414,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Saskatchewan, 45 MPa",474,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Saskatchewan, 45 MPa, w/o AEAs",458,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 20 MPa",204,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 20 MPa, w/o AEAs",202,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 25 MPa",230,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 25 MPa, w/o AEAs",223,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 30 MPa",253,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 30 MPa, w/o AEAs",246,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 32 MPa",277,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 35 MPa",298,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 35 MPa, w/o AEAs",268,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 40 MPa",309,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 40 MPa, w/o AEAs",290,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 45 MPa",362,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 45 MPa, w/o AEAs",333,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 50 MPa",396,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Manitoba, 50 MPa, w/o AEAs",367,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 20 MPa",227,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 20 MPa, w/o AEAs",220,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 25 MPa",261,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 25 MPa, w/o AEAs",254,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 30 MPa",293,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 30 MPa, w/o AEAs",264,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 32 MPa",326,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 32 MPa, w/o AEAs",264,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 35 MPa",334,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 35 MPa, w/o AEAs",295,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 40 MPa",362,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 40 MPa, w/o AEAs",326,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 45 MPa, w/ AEAs",379,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 45 MPa",350,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 50 MPa, w/ AEAs",457,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 50 MPa",336,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 55 MPa",355,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 60 MPa",361,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Ontario, 70 MPa",354,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 20 MPa",278,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 20 MPa, w/o AEAs",264,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 25 MPa",299,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 25 MPa, w/o AEAs",287,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 30 MPa",343,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 30 MPa, w/o AEAs",307,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 32 MPa",363,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 35 MPa, w/ AEAs",393,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 35 MPa",345,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 40 MPa, w/ AEAs",397,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 40 MPa",364,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 45 MPa, w/ AEAs",414,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 45 MPa",381,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 50 MPa, w/ AEAs",411,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 50 MPa",404,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 60 MPa, w/ AEAs",445,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 60 MPa",425,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Quebec, 80 MPa, w/o AEAs",486,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 20 MPa, w/ AEAs",344,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 20 MPa",337,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 25 MPa, w/ AEAs",361,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 25 MPa",354,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 30 MPa, w/ AEAs",394,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 30 MPa",379,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 32 MPa, w/ AEAs",439,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 35 MPa, w/ AEAs",447,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 35 MPa",422,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 40 MPa, w/ AEAs",474,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 40 MPa",449,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 45 MPa, w/ AEAs",529,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 45 MPa",502,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 50 MPa, w/ AEAs",551,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 50 MPa",536,"1 m3"]
[null,"Ready-mix","Ready-mixed concrete, Canada, Atlantic, 60 MPa, w/o AEAs",580,"1 m3"]
[null,"Shotcrete","Shotcrete, U.S. Pacific Southwest, 4000 psi",375,"1 m3"]
[null,"Shotcrete","Shotcrete, U.S. Pacific Southwest, 5000 psi",439,"1 m3"]
[null,"Shotcrete","Shotcrete, U.S. Pacific Southwest, 6000 psi",442,"1 m3"]
[null,"Shotcrete","Shotcrete, U.S. Pacific Northwest, 4000 psi",362,"1 m3"]
[null,"Shotcrete","Shotcrete, U.S. Pacific Northwest, 5000 psi",411,"1 m3"]
[null,"Shotcrete","Shotcrete, U.S. Pacific Northwest, 6000 psi",402,"1 m3"]
[null,"Shotcrete","Shotcrete, British Columbia, 35 MPa",300,"1 m3"]
[null,"Shotcrete","Shotcrete, British Columbia, 40 MPa",313,"1 m3"]
[null,"Shotcrete","Shotcrete, British Columbia, 45 MPa",337,"1 m3"]
[null,"Concrete masonry units","CMU, USA, normal weight, f'm=2000psi",208,"1 m3"]
[null,"Concrete masonry units","CMU, USA, normal weight, f'm=2500psi",232,"1 m3"]
[null,"Concrete masonry units","CMU, USA, normal weight, f'm=3000psi",241,"1 m3"]
[null,"Concrete masonry units","CMU, USA, medium weight, manufactured aggregate",360,"1 m3"]
[null,"Concrete masonry units","CMU, USA, medium weight, natural aggregate and industrial byproducts",244,"1 m3"]
[null,"Concrete masonry units","CMU, USA, medium weight",300,"1 m3"]
[null,"Concrete masonry units","CMU, USA, lightweight, manufactured aggregate",395,"1 m3"]
[null,"Concrete masonry units","CMU, USA, lightweight, natural aggregate and industrial byproducts",286,"1 m3"]
[null,"Concrete masonry units","CMU, USA, lightweight",340,"1 m3"]
[null,"Concrete masonry units","CMU, Eastern Canada, normal weight (all cement types)",200,"1 m3"]
[null,"Concrete masonry units","CMU, Eastern Canada, normal weight, GU SCM",205,"1 m3"]
[null,"Concrete masonry units","CMU, Eastern Canada, normal weight, GUL SCM",191,"1 m3"]
[null,"Concrete masonry units","CMU, Eastern Canada, lightweight (all cement types)",170,"1 m3"]
[null,"Concrete masonry units","CMU, Eastern Canada, lightweight, GU SCM",177,"1 m3"]
[null,"Concrete masonry units","CMU, Eastern Canada, lightweight, GUL SCM",164,"1 m3"]
[null,"Concrete masonry units","CMU, Western Canada, normal weight (all cement types)",240,"1 m3"]
[null,"Concrete masonry units","CMU, Western Canada, normal weight, GU SCM",252,"1 m3"]
[null,"Concrete masonry units","CMU, Western Canada, normal weight, GUL SCM",232,"1 m3"]
[null,"Concrete masonry units","CMU, Western Canada, lightweight (all cement types)",210,"1 m3"]
[null,"Concrete masonry units","CMU, Western Canada, lightweight, GU SCM",214,"1 m3"]
[null,"Concrete masonry units","CMU, Western Canada, lightweight, GUL SCM",198,"1 m3"]
[null,"Brick","Clay brick",503,"1 m3"]
[null,"Rebar","Rebar, unfabricated",753,"1 metric ton"]
[null,"Rebar","Rebar, fabricated",854,"1 metric ton"]
[null,"Structural steel","Hot-rolled sections, unfabricated",901,"1 metric ton"]
[null,"Structural steel","Hot-rolled sections, fabricated",1080,"1 metric ton"]
[null,"Structural steel","Steel plate, unfabricated",1480,"1 metric ton"]
[null,"Structural steel","Steel plate, fabricated",1730,"1 metric ton"]
[null,"Structural steel","HSS, unfabricated",1710,"1 metric ton"]
[null,"Structural steel","HSS, fabricated",1990,"1 metric ton"]
[null,"Cold-formed steel framing","Cold-formed steel framing",2440,"1 metric ton"]
[null,"Steel decking","Steel deck",2330,"1 metric ton"]
[null,"Open-web steel joists","Open-web steel joist",1430,"1 metric ton"]
[null,"Aluminum extrusions ","Aluminum extrusions, mill finish",10300,"1 metric ton"]
[null,"Aluminum extrusions ","Aluminum extrusions, anodized",10800,"1 metric ton"]
[null,"Aluminum extrusions ","Aluminum extrusions, painted",11700,"1 metric ton"]
[null,"Aluminum extrusions ","Aluminum extrusions, thermally improved, anodized",11800,"1 metric ton"]
[null,"Aluminum extrusions ","Aluminum extrusions, thermally improved, painted",12700,"1 metric ton"]
[null,"Aluminum sheet","Aluminum sheet",3820,"1 metric ton"]
[null,"Sawn lumber","Softwood Lumber",63.1,"1 m3"]
[null,"Sawn lumber","Softwood lumber, U.S. Inland Northwest",71.400000000000006,"1 m3"]
[null,"Sawn lumber","Softwood lumber, U.S. Southern",90.4,"1 m3"]
[null,"Sawn lumber","Softwood lumber, U.S. Pacific Coast",73.8,"1 m3"]
[null,"Sawn lumber","Softwood lumber, British Columbia",45.9,"1 m3"]
[null,"Sawn lumber","Redwood Lumber",38,"1 m3"]
[null,"Structural composite lumber ","Laminated strand lumber (LSL)",275,"1 m3"]
[null,"Structural composite lumber ","Laminated veneer lumber (LVL)",361,"1 m3"]
[null,"Mass timber","Cross laminated timber (CLT), North America",134,"1 m3"]
[null,"Mass timber","CLT, British Columbia",101,"1 m3"]
[null,"Mass timber","CLT, Eastern Canada",96,"1 m3"]
[null,"Mass timber","CLT, Southern US",147,"1 m3"]
[null,"Mass timber","CLT, Western US",156,"1 m3"]
[null,"Mass timber","Mass ply panel (MPP)",259,"1 m3"]
[null,"Mass timber","Dowel Laminated Timber (DLT)",121,"1 m3"]
[null,"Mass timber","Glue laminated timber (GLT)",137,"1 m3"]
[null,"Mass timber","GLT, British Columbia",103,"1 m3"]
[null,"Wood sheathing ","Softwood plywood",219,"1 m3"]
[null,"Wood sheathing ","Softwood plywood, British Columbia",132,"1 m3"]
[null,"Wood sheathing ","Oriented strandboard (OSB)",243,"1 m3"]
[null,"Wood sheathing ","Wood sheathing (includes plywood and OSB)",231,"1 m3"]
[null,"Wood I-joists","Wood I-joist, 300mm (≅11-7/8\")",1.97,"1 m"]
[null,"Board insulation ","Expanded polystyrene (EPS) Type I",2.5299999999999998,"1 m2@RSI-1"]
[null,"Board insulation ","Fiberglass board",5.0199999999999996,"1 m2@RSI-1"]
[null,"Board insulation ","Heavy density mineral wool board",6.82,"1 m2@RSI-1"]
[null,"Board insulation ","Polyiso, aluminum foil facer",4.0999999999999996,"1 m2@RSI-1"]
[null,"Board insulation ","Polyiso, GRF facer",2.11,"1 m2@RSI-1"]
[null,"Board insulation ","Polyiso, CGF facer",2.95,"1 m2@RSI-1"]
[null,"Board insulation ","Polyiso, wall",3.5,"1 m2@RSI-1"]
[null,"Board insulation ","Polyiso, roof",2.5,"1 m2@RSI-1"]
[null,"Board insulation ","Extruded polystyrene (XPS) board, ≤25 psi",8.9,"1 m2@RSI-1"]
[null,"Board insulation ","Extruded polystyrene (XPS) board, 40 psi",10.9,"1 m2@RSI-1"]
[null,"Board insulation ","Extruded polystyrene (XPS) board, 60 psi",14.1,"1 m2@RSI-1"]
[null,"Board insulation ","Extruded polystyrene (XPS) board, 100 psi",20.100000000000001,"1 m2@RSI-1"]
[null,"Blanket insulation ","Fiberglass blanket",1.06,"1 m2@RSI-1"]
[null,"Blanket insulation ","Mineral wool blanket",2.68,"1 m2@RSI-1"]
[null,"Blanket insulation ","Blanket insulation (general)",1.9,"1 m2@RSI-1"]
[null,"Foamed-in-place insulation ","Closed-cell spray polyurethane foam, medium density",2.63,"1 m2@RSI-1"]
[null,"Foamed-in-place insulation ","Closed-cell spray polyurethane foam, roofing",3.87,"1 m2@RSI-1"]
[null,"Foamed-in-place insulation ","Open-cell spray polyurethane foam",1.17,"1 m2@RSI-1"]
[null,"Loose-fill insulation ","Mineral wool loose fill",1.89,"1 m2@RSI-1"]
[null,"Loose-fill insulation ","Fiberglass loose fill",0.98799999999999999,"1 m2@RSI-1"]
[null,"Loose-fill insulation ","Cellulose loose fill",0.48699999999999999,"1 m2@RSI-1"]
[null,"Loose-fill insulation ","Loose-fill insulation (all types)",1.1000000000000001,"1 m2@RSI-1"]
[null,"Applied fireproofing","Spray-applied fireproofing, standard density",388,"1 metric ton"]
[null,"Applied fireproofing","Spray-applied fireproofing, medium density",749,"1 metric ton"]
[null,"Applied fireproofing","Spray-applied fireproofing, high density",902,"1 metric ton"]
[null,"Metal panel cladding ","Roll-formed metal panel - steel",1530,"100 m2"]
[null,"Metal panel cladding ","Roll-formed metal panel - aluminum",1860,"100 m2"]
[null,"Metal panel cladding ","Roll-formed metal panel (all)",1700,"100 m2"]
[null,"Metal panel cladding ","MCM panel, aluminum",2800,"100 m2"]
[null,"Insulated metal panel cladding ","Insulated metal panel (IMP), 2\" thick",10700,"100 m2"]
[null,"Insulated metal panel cladding ","Insulated metal panel (IMP), 4\" thick",19100,"100 m2"]
[null,"Insulated metal panel cladding ","Insulated metal panel (IMP), 6\" thick",27400,"100 m2"]
[null,"Insulated metal panel cladding ","Insulated metal panel (IMP), user-defined thickness","[user- calculated]","100 m2"]
[null,"Membrane roofing ","Built-up asphalt roofing (BUR), Hot Asphalt        ",2.57,"1 m2"]
[null,"Membrane roofing ","BUR, Fastened Base, 2 Ply Felts and Cap in Hot Asphalt\n",3.06,"1 m2"]
[null,"Membrane roofing ","SBS-modified bitumen roofing membrane, installation: cold adhesive",5.81,"1 m2"]
[null,"Membrane roofing ","SBS-modified bitumen roofing membrane, installation: hot asphalt",5.81,"1 m2"]
[null,"Membrane roofing ","SBS-modified bitumen roofing membrane, installation: hybrid self-adhered SBS base sheet and torch-applied SBS cap",5.54,"1 m2"]
[null,"Membrane roofing ","SBS-modified bitumen roofing membrane, installation: self adhered",5.2,"1 m2"]
[null,"Membrane roofing ","SBS-modified bitumen roofing membrane, installation: torch applied",5.85,"1 m2"]
[null,"Membrane roofing ","SBS-modified bitumen roofing membrane",5.64,"1 m2"]
[null,"Membrane roofing ","APP-modified bitumen roofing membrane, installation: cold adhesive",9.2200000000000006,"1 m2"]
[null,"Membrane roofing ","APP-modified bitumen roofing membrane, installation: torch applied:",9.01,"1 m2"]
[null,"Membrane roofing ","APP-modified bitumen roofing membrane",9.1199999999999992,"1 m2"]
[null,"Membrane roofing ","SBS/APP-modified bitumen roofing membrane, hybrid self-adhered SBS base sheet and torch-applied APP",5.13,"1 m2"]
[null,"Membrane roofing ","Single ply PVC membrane roofing, 40 mils",4.2,"1 m2"]
[null,"Membrane roofing ","Single ply PVC membrane roofing, 48 mils",5.2,"1 m2"]
[null,"Membrane roofing ","Single ply PVC membrane roofing, 60 mils",6.3,"1 m2"]
[null,"Membrane roofing ","Single ply PVC membrane roofing, 80 mils",8.3000000000000007,"1 m2"]
[null,"Membrane roofing ","TPO membrane roofing, 45 mil",3.32,"1 m2"]
[null,"Membrane roofing ","TPO membrane roofing, 60 mil",4.29,"1 m2"]
[null,"Membrane roofing ","TPO membrane roofing, 80 mil",6.05,"1 m2"]
[null,"Membrane roofing ","EPDM membrane roofing, reinforced, 45 mil",5.42,"1 m2"]
[null,"Membrane roofing ","EPDM membrane roofing, reinforced, 60 mil",7.1,"1 m2"]
[null,"Membrane roofing ","EPDM membrane roofing, reinforced, 75 mil",8.86,"1 m2"]
[null,"Membrane roofing ","EPDM membrane roofing, non-reinforced, 45 mil",4.7300000000000004,"1 m2"]
[null,"Membrane roofing ","EPDM membrane roofing, non-reinforced, 60 mil",6.14,"1 m2"]
[null,"Membrane roofing ","EPDM membrane roofing, non-reinforced, 90 mil",9.56,"1 m2"]
[null,"Asphalt shingles","Asphalt shingles",3.61,"1 m2"]
[null,"Flat glass ","Flat glass",1430,"1 metric ton"]
[null,"Asphalt mixtures","Aspalt mixtures [multiple; see category results in report]","[see category results in report]","1 metric ton"]